##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99136.4mmHXHT.27072021.7Li.Li6.5P0.5Si0.5O5Cl/9/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-27 13:00:41.936 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-27 12:59:45.154 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 6218
       D7 D3 C7 99 FD 61 95 36 16 3F 35 CB 86 0B 84 3D>)
(   2,<2021-07-27 13:01:00.978 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 180 FT_mod = 6 PKNL = 1 PHC0 = 211.3882 PHC1 = -46.8523 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       3F 61 E9 2C BF 36 2D B3 82 9D 42 8F 8B 96 A7 E5>)
(   3,<2021-07-27 13:01:08.775 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.5P0.5Si0.5O5Cl
       L6.5P0.5S0.5O5Cl_17
       Ref Static
       4mm HXHT Probe
       sr = -813.97 Hz
       90 deg at 2.2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 302 K
       
       
       
       Tsensor = 342 K
       heater = 1 %
       gasflow= 3000 l/h
       bp = 2500 mbar
       Tsample = 330 K
       
       fwhm = 1825 HzTITLE_END
       data hash MD5: 8K
       3F 61 E9 2C BF 36 2D B3 82 9D 42 8F 8B 96 A7 E5>)
(   4,<2021-07-27 13:01:09.075 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.5P0.5Si0.5O5Cl
       L6.5P0.5S0.5O5Cl_17
       Ref Static
       4mm HXHT Probe
       sr = -813.97 Hz
       90 deg at 2.2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 302 K
       
       
       
       Tsensor = 342 K
       heater = 1 %
       gasflow= 3000 l/h
       bp = 2500 mbar
       Tsample = 330 K
       
       fwhm = 1825 HzTITLE_END
       data hash MD5: 8K
       3F 61 E9 2C BF 36 2D B3 82 9D 42 8F 8B 96 A7 E5>)
##END=

$$ hash MD5
$$ 51 77 A0 E3 4F B6 45 16 B1 C8 2E 74 2D E4 8E 90
