##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99137.4mmHXHT.27072021.7Li.Li7SiO5Cl/18/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-28 15:44:53.054 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-28 15:43:32.278 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 6218
       56 2B 82 D8 9F 92 92 39 CE 29 C3 4A 93 CB 74 F3>)
(   2,<2021-07-28 15:52:03.765 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 150 FT_mod = 6 PKNL = 1 PHC0 = -194.2443 PHC1 = 25.753 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       C1 BE F7 0D 6D BA 8A F1 20 41 F0 5D C8 05 4D A4>)
(   3,<2021-07-28 15:52:10.072 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 306 K
       
       
       
       Tsensor = 415.5 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 380 K
       
       fwhm = 1500 HzTITLE_END
       data hash MD5: 8K
       C1 BE F7 0D 6D BA 8A F1 20 41 F0 5D C8 05 4D A4>)
(   4,<2021-07-28 15:52:10.468 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 306 K
       
       
       
       Tsensor = 415.5 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 380 K
       
       fwhm = 1500 HzTITLE_END
       data hash MD5: 8K
       C1 BE F7 0D 6D BA 8A F1 20 41 F0 5D C8 05 4D A4>)
##END=

$$ hash MD5
$$ E6 8B 0F 8D 3A 2A 3B 82 BF 57 C2 95 E2 98 64 47
