##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99137.4mmHXHT.27072021.7Li.Li7SiO5Cl/6/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-28 13:27:40.272 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-28 13:20:59.501 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 6218
       8C D3 1A 64 20 3C 61 4E 1F C9 DB BB 2C 24 40 16>)
(   2,<2021-07-28 13:54:45.315 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 850 FT_mod = 6 PKNL = 1 PHC0 = -181.8443 PHC1 = 25.753 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       3C 74 EF 9B 30 A8 C3 F6 5F DE 3A DA B6 94 95 00>)
(   3,<2021-07-28 13:54:53.774 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 302 K
       
       
       
       Tsensor = 327 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 320 K
       
       fwhm = 8600 HzTITLE_END
       data hash MD5: 8K
       3C 74 EF 9B 30 A8 C3 F6 5F DE 3A DA B6 94 95 00>)
(   4,<2021-07-28 13:54:53.970 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 302 K
       
       
       
       Tsensor = 327 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 320 K
       
       fwhm = 8600 HzTITLE_END
       data hash MD5: 8K
       3C 74 EF 9B 30 A8 C3 F6 5F DE 3A DA B6 94 95 00>)
##END=

$$ hash MD5
$$ 66 06 43 73 C4 7A AC 3E 61 63 C6 73 7A CF 0E 13
