##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99136.4mmHXHT.27072021.7Li.Li6.5P0.5Si0.5O5Cl/5/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-27 12:16:08.830 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-27 12:14:48.065 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 6218
       21 9C DD 0E 79 8D 64 8A 8D FC FE D6 BE D4 06 59>)
(   2,<2021-07-27 12:16:22.248 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 350 FT_mod = 6 PKNL = 1 PHC0 = 213.1882 PHC1 = -46.8523 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       68 67 27 E8 FA 94 36 18 FB 82 4D 8E B7 F7 48 47>)
(   3,<2021-07-27 12:16:30.764 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.5P0.5Si0.5O5Cl
       L6.5P0.5S0.5O5Cl_17
       Ref Static
       4mm HXHT Probe
       sr = -813.97 Hz
       90 deg at 2.2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 302 K
       
       
       
       Tsensor = 312.5 K
       heater = 1 %
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 310 K
       
       fwhm = 3400 HzTITLE_END
       data hash MD5: 8K
       68 67 27 E8 FA 94 36 18 FB 82 4D 8E B7 F7 48 47>)
(   4,<2021-07-27 12:16:31.232 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.5P0.5Si0.5O5Cl
       L6.5P0.5S0.5O5Cl_17
       Ref Static
       4mm HXHT Probe
       sr = -813.97 Hz
       90 deg at 2.2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 302 K
       
       
       
       Tsensor = 312.5 K
       heater = 1 %
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 310 K
       
       fwhm = 3400 HzTITLE_END
       data hash MD5: 8K
       68 67 27 E8 FA 94 36 18 FB 82 4D 8E B7 F7 48 47>)
##END=

$$ hash MD5
$$ B9 8A 62 BC DB 9A F4 CB 4D F4 73 E6 BD F8 AA A5
