##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99137.4mmHXHT.27072021.7Li.Li7SiO5Cl/26/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-28 17:19:16.657 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-28 17:18:43.891 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 6218
       E5 D1 83 4E 52 E2 E5 38 A1 21 EB 07 03 FC 96 F7>)
(   2,<2021-07-28 17:25:00.239 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 70 FT_mod = 6 PKNL = 1 PHC0 = -184.5524 PHC1 = 16.78572 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       54 87 DD 44 BF 99 7E 83 0C D1 85 31 76 5B 19 5E>)
(   3,<2021-07-28 17:25:07.586 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 308 K
       
       
       
       Tsensor = 481.6 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 425 K
       
       fwhm = 680 HzTITLE_END
       data hash MD5: 8K
       54 87 DD 44 BF 99 7E 83 0C D1 85 31 76 5B 19 5E>)
(   4,<2021-07-28 17:25:07.868 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 308 K
       
       
       
       Tsensor = 481.6 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 425 K
       
       fwhm = 680 HzTITLE_END
       data hash MD5: 8K
       54 87 DD 44 BF 99 7E 83 0C D1 85 31 76 5B 19 5E>)
##END=

$$ hash MD5
$$ E2 D4 3F 08 E6 ED 8A 5A 36 38 37 B7 19 FC AD 80
