##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99137.4mmHXHT.27072021.7Li.Li7SiO5Cl/32/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-28 18:23:50.169 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-28 18:23:17.399 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 6218
       7A 83 28 32 45 D9 28 A0 8D 58 50 04 04 44 2C C9>)
(   2,<2021-07-28 18:24:00.097 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 55 FT_mod = 6 PKNL = 1 PHC0 = -191.7766 PHC1 = 9.275293 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       F1 5B D6 BD C9 54 24 17 4F C8 4C 17 E2 50 E6 5F>)
(   3,<2021-07-28 18:24:06.364 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 315 K
       
       
       
       Tsensor = 592 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 500 K
       
       fwhm = 550 HzTITLE_END
       data hash MD5: 8K
       F1 5B D6 BD C9 54 24 17 4F C8 4C 17 E2 50 E6 5F>)
(   4,<2021-07-28 18:24:06.562 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 315 K
       
       
       
       Tsensor = 592 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 500 K
       
       fwhm = 550 HzTITLE_END
       data hash MD5: 8K
       F1 5B D6 BD C9 54 24 17 4F C8 4C 17 E2 50 E6 5F>)
##END=

$$ hash MD5
$$ 2B 2B 9B 5A 61 2B 60 73 8D 2C 33 97 3A DA BE FB
