##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99138.4mmHXY.30072021.7Li.Li7SiO5Cl/12/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-30 14:28:22.416 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-30 14:19:01.648 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 4664
       26 2D 59 2F D0 59 09 B3 CB 03 A3 0D 27 68 44 EB>)
(   2,<2021-07-30 14:30:00.653 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 1020 FT_mod = 6 PKNL = 1 PHC0 = -154.4618 PHC1 = -2.850697 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       05 B4 FF FA D7 A5 54 C8 9A 1F 66 E6 36 16 33 1F>)
(   3,<2021-07-30 14:30:08.375 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <pk fgphup PHC0 = -7.205274 PHC1 = 14.4 
       data hash MD5: 8K
       FA 8D AE 8E 4C 4D 3A B2 43 DF B0 E3 B3 81 3E B8>)
(   4,<2021-07-30 14:30:18.464 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Static
       4mm HXY Probe
       sr = -915.53Hz
       90 deg at 2 us ( 83 kHz) at 68 W
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 296 K
       
       
       
       Tsensor = 250 K
       gasflow= 400 l/h
       Tsample = 240 K
       
       fwhm = 10250 HzTITLE_END
       data hash MD5: 8K
       FA 8D AE 8E 4C 4D 3A B2 43 DF B0 E3 B3 81 3E B8>)
(   5,<2021-07-30 14:30:18.773 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Static
       4mm HXY Probe
       sr = -915.53Hz
       90 deg at 2 us ( 83 kHz) at 68 W
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 296 K
       
       
       
       Tsensor = 250 K
       gasflow= 400 l/h
       Tsample = 240 K
       
       fwhm = 10250 HzTITLE_END
       data hash MD5: 8K
       FA 8D AE 8E 4C 4D 3A B2 43 DF B0 E3 B3 81 3E B8>)
##END=

$$ hash MD5
$$ 6E F9 E8 E0 EC EE A9 16 70 BA 2B 69 2D 74 31 A2
