##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99137.4mmHXHT.27072021.7Li.Li7SiO5Cl/30/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-28 18:01:14.469 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-28 18:00:41.693 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 6218
       B4 88 21 CB E7 FD 8B 17 8D F7 F7 78 1D 12 11 BC>)
(   2,<2021-07-28 18:08:34.130 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 60 FT_mod = 6 PKNL = 1 PHC0 = -198.9898 PHC1 = 36.33299 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       33 52 04 10 8E 6A DE 14 25 E7 4C 14 AC E1 A8 60>)
(   3,<2021-07-28 18:08:40.470 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 312 K
       
       
       
       Tsensor = 548 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 470 K
       
       fwhm = 620 HzTITLE_END
       data hash MD5: 8K
       33 52 04 10 8E 6A DE 14 25 E7 4C 14 AC E1 A8 60>)
(   4,<2021-07-28 18:08:40.843 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Ref Static
       4mm HXHT Probe
       sr = -915.53 Hz
       90 deg at 2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 312 K
       
       
       
       Tsensor = 548 K
       gasflow= 3000 l/h
       bp = 1500 mbar
       Tsample = 470 K
       
       fwhm = 620 HzTITLE_END
       data hash MD5: 8K
       33 52 04 10 8E 6A DE 14 25 E7 4C 14 AC E1 A8 60>)
##END=

$$ hash MD5
$$ 52 0B C8 70 DF 7B 75 B0 37 F2 AA 42 0F 01 39 43
