##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99148.4mmHXY.07122021.7Li.Li6.3P0.7S0.3O5Cl/7/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-12-10 11:27:35.986 +0000>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-12-10 11:24:55.140 +0000,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       14 DF 9F FE 32 6F C1 BE 6E 3D AE 20 D0 87 06 96
       data hash MD5: 9350
       63 8A 4C DD 3B 2C F0 0E 84 96 B8 C2 E8 AF BE B8>)
(   2,<2021-12-10 12:08:57.254 +0000>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 700 FT_mod = 6 PKNL = 1 PHC0 = 202.0083 PHC1 = -37.44243 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       94 CB 52 E9 EE F9 3A AE 55 8B 6B 7D E3 7D 2D F4>)
(   3,<2021-12-10 12:09:05.346 +0000>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <pk fgphup PHC0 = 20.8 PHC1 = 0 
       data hash MD5: 8K
       C6 9E C7 0B B8 25 21 24 B1 00 FF A7 DF 72 01 40>)
(   4,<2021-12-10 12:09:14.093 +0000>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.3P0.7S0.3O5Cl
       Li6.3P0.7S0.3O5Cl_12
       Static
       4mm HXY Probe
       sr = -772.55 Hz
       90 deg  us 83 kHz at 68.3 W
       
       frame cooling = 70 %
       magnet cooling = 13 turns (full)
       Tshim = 294 K
       
       
       
       Tsensor = 272 K
       Gas flow = 600 l/ph
       Tsample = 265 K
       
       fwhm = 6950 HzTITLE_END
       data hash MD5: 8K
       C6 9E C7 0B B8 25 21 24 B1 00 FF A7 DF 72 01 40>)
(   5,<2021-12-10 12:09:14.311 +0000>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.3P0.7S0.3O5Cl
       Li6.3P0.7S0.3O5Cl_12
       Static
       4mm HXY Probe
       sr = -772.55 Hz
       90 deg  us 83 kHz at 68.3 W
       
       frame cooling = 70 %
       magnet cooling = 13 turns (full)
       Tshim = 294 K
       
       
       
       Tsensor = 272 K
       Gas flow = 600 l/ph
       Tsample = 265 K
       
       fwhm = 6950 HzTITLE_END
       data hash MD5: 8K
       C6 9E C7 0B B8 25 21 24 B1 00 FF A7 DF 72 01 40>)
##END=

$$ hash MD5
$$ 8E 83 82 BB 50 16 67 4D 7B 5C 35 34 59 B6 EC 77
