##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99148.4mmHXY.07122021.7Li.Li6.3P0.7S0.3O5Cl/25/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-12-10 16:33:06.561 +0000>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-12-10 16:25:45.609 +0000,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       14 DF 9F FE 32 6F C1 BE 6E 3D AE 20 D0 87 06 96
       data hash MD5: 9350
       9C 72 7B CA 8C B2 BA 2F C4 FE 8B F4 C7 42 99 D4>)
(   2,<2021-12-10 16:33:45.841 +0000>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 920 FT_mod = 6 PKNL = 1 PHC0 = 215.6083 PHC1 = -37.44243 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       47 81 51 07 A1 93 21 AA C2 B3 4C D5 FD 62 68 F0>)
(   3,<2021-12-10 16:34:02.105 +0000>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <pk fgphup PHC0 = 5.4 PHC1 = 0 
       data hash MD5: 8K
       D7 D0 D5 FB A1 50 E9 6F 9F 05 C0 47 31 8D 24 04>)
(   4,<2021-12-10 16:34:14.243 +0000>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.3P0.7S0.3O5Cl
       Li6.3P0.7S0.3O5Cl_12
       Static
       4mm HXY Probe
       sr = -772.55 Hz
       90 deg  us 83 kHz at 68.3 W
       
       frame cooling = 70 %
       magnet cooling = 13 turns (full)
       Tshim = 290 K
       
       
       
       Tsensor = 172 K
       Gas flow = 600 l/ph
       Tsample = 150 K
       
       fwhm = 9275 HzTITLE_END
       data hash MD5: 8K
       D7 D0 D5 FB A1 50 E9 6F 9F 05 C0 47 31 8D 24 04>)
(   5,<2021-12-10 16:34:14.574 +0000>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.3P0.7S0.3O5Cl
       Li6.3P0.7S0.3O5Cl_12
       Static
       4mm HXY Probe
       sr = -772.55 Hz
       90 deg  us 83 kHz at 68.3 W
       
       frame cooling = 70 %
       magnet cooling = 13 turns (full)
       Tshim = 290 K
       
       
       
       Tsensor = 172 K
       Gas flow = 600 l/ph
       Tsample = 150 K
       
       fwhm = 9275 HzTITLE_END
       data hash MD5: 8K
       D7 D0 D5 FB A1 50 E9 6F 9F 05 C0 47 31 8D 24 04>)
##END=

$$ hash MD5
$$ 1A 0B A2 8D E5 81 DE CF A1 E0 74 FB A3 E5 BE 9D
