Data was collected at 100 K with a Rigaku MicroMax-007 HF X-ray generator equipped with a Mo Ka rotating-anode microfocus source and a Saturn 724+ detector. The data was processed using CrysAlisPro software package.
 
Single crystal data (raw detector images) in Rigaku .img format
Files are readable in Rigaku's CrysAlis(Pro) program which can be obtained free of charge upon registration at http://www.rigakuxrayforum.com/
