Synchrotron powder XRD was performed at the I11 beamline at Diamond Light Source (Oxfordshire, U.K.), with an incident wavelength 
of 0.825949 Å using a wide-angle position sensitive (PSD) detector and samples sealed in Ø = 0.5 mm borosilicate glass capillaries.
The synchrotron data is in .xye format and presented in a 3 column: 2Theta, counts and error.
Lab data was carried out using Rigaku SmartLab diffractometer with monochromatic Mo radiation (Kα1, λ = 0.7093 Å) 
and Bruker D8 Discover diffractometer with monochromatic Cu radiation (Kα1, λ = 1.540596 Å) in Debye−Scherrer transmission geometry.
The Lab data is in .raw format.