Galvanostatic Cycling with Potential Limitation

Run on channel : 6 (SN 11395)
User : 
Electrode connection : standard
Potential control : Ewe
Ewe ctrl range : min = -10.00 V, max = 10.00 V
Ewe,I filtering : <None>
Safety Limits :
	Do not start on E overload
Channel : Floating
Acquisition started on : 04/01/2022 13:31:13.000
Loaded Setting File : NONE
Saved on :
	File : plating-283-c-RT-50 uA cm-2-0.98mm_0.196cm2-1_02_GCPL_C06.mpr
	Directory : C:\Users\mjr\Documents\EC-Lab\Data\Guopeng\LiSiSI\283-c\
	Host : 138.253.124.214
Device : VSP-300 (SN 0655)
Address : 138.253.124.215
EC-Lab for windows v11.27 (software)
Internet server v11.25 (firmware)
Command interpretor v11.27 (firmware)
Electrode material : Au/Pd
Initial state : 
Electrolyte : NaCl (0.2M)
Comments : Fe(CN)63-/Fe(CN)64- 5.10-3 M
Mass of active material : 0.001 mg
 at x = 0.000
Molecular weight of active material (at x = 0) : 0.001 g/mol
Atomic weight of intercalated ion : 0.001 g/mol
Acquisition started at : xo = 0.000
Number of e- transfered per intercalated ion : 1
for DX = 1, DQ = 26.802 mA.h
Battery capacity : 0.000 A.h
Cable : ULC
Reference electrode : SCE Saturated Calomel Electrode (0.241 V)
Electrode surface area : 0.001 cm²
Characteristic mass : 0.001 g
Volume (V) : 0.000 m³
Cycle Definition : Charge/Discharge alternance
Ns                  0                   1                   2                   
Set I/C             I                   I                   I                   
Is                  0.000               9.817               -9.817              
unit Is             mA                  µA                  µA                  
vs.                 <None>              <None>              <None>              
N                   1.00                1.00                1.00                
I sign              > 0                 > 0                 > 0                 
t1 (h:m:s)          0:00:0.0000         0:30:0.0000         0:30:0.0000         
I Range             10 µA               10 µA               10 µA               
Bandwidth           5                   5                   5                   
dE1 (mV)            0.00                5.00                5.00                
dt1 (s)             0.0000              5.0000              5.0000              
EM (V)              0.000               4.500               -4.500              
tM (h:m:s)          0:00:0.0000         0:00:0.0000         0:00:0.0000         
Im                  0.000               0.000               0.000               
unit Im             mA                  mA                  mA                  
dI/dt               0.000               0.000               0.000               
dunit dI/dt         mA/s                mA/s                mA/s                
E range min (V)     -10.000             -10.000             -10.000             
E range max (V)     10.000              10.000              10.000              
dq                  0.000               1.000               1.000               
unit dq             A.h                 A.h                 A.h                 
dtq (s)             0.0000              120.0000            120.0000            
dQM                 0.000               0.000               0.000               
unit dQM            mA.h                mA.h                mA.h                
dxM                 0.000               0.000               0.000               
delta SoC (%)       pass                pass                pass                
tR (h:m:s)          0:00:0.0000         0:00:0.0000         0:00:0.0000         
dER/dt (mV/h)       0.0                 0.1                 0.1                 
dER (mV)            0.00                0.00                0.00                
dtR (s)             1.0000              120.0000            120.0000            
EL (V)              pass                4.200               4.200               
goto Ns'            0                   0                   1                   
nc cycles           0                   0                   2000                
