TITLE=MW OFF
Probe: 3.2 mm DNP HCN mode, AVNeo console
Sample: sample 9 HPMC-AS (HF) repeat
Saphire rotor
MAS = 8 kHz, BP = 2660 mB, DP = 1091 mB
Tsample = 121.4 K, flow = 2000 l/h, Heater 0%, Tbearing = 130.5 K, Heater 13.6%, Tdrive = 130.4 K, Heater 10.5%
13C CP echo no filter

1H pulses and SPINAL dec 100 kHz at 67 W, o2 1H offset = -64442 Hz, pcpd2 = 4.8 us
1H CP 100 kHz matched to 13C at 60 W (71 kHz), ramp 70.100.100 on 1H
1 ms CP
L0 = 3
At temp in file 69TITLE_END