CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Thu Feb 15 08:47:46 2024
Release      : TopSpin 4.3.0
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.3.180.20230524
CPU          : Intel(R) Core(TM) i7-4700EQ CPU @ 2.40GHz (8 cores at 2210 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 400 NMR spectrometer
1H-frequency : 400.27 MHz
Description  : Avance Neo
Bruker Order : 419051
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- EPU/2: AV4 EPU/2 Embedded Processing Unit H153448F1/01462 ECL 01.04
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/04652 ECL 02.03
  Location: slot 1 in rack 1
  Connection: at IP 192.168.180.14 via PCIe #3
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd2, DRX at /dev/bbu/drx3.5, RTD at /dev/bbu/rtd3.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/04654 ECL 02.03
  Location: slot 2 in rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd11, DRX at /dev/bbu/drx4.5, RTD at /dev/bbu/rtd4.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/04653 ECL 02.03
  Location: slot 3 in rack 1
  Connection: at IP 192.168.180.22 via PCIe #5
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd20, DRX at /dev/bbu/drx5.5, RTD at /dev/bbu/rtd5.4
  Sequencer: FCube
  - FCube3
- GTU: AV4 GT-CONTROLLER UNIT Z148393/01496 ECL 01.02
  Location: slot 6 in rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20190906085855
  - Gradient resolution: 1.0 us
  Devices: MTD at /dev/mtd28, RTD at /dev/bbu/rtd9.4, GPROC at /dev/bbu/gproc9.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- PSM-A: AV4 PSM-A Z149510/02025 ECL 03.01
- HPPR/2 COVER2: HPPR/2 Cover2 Z124567/03529 ECL 00.05
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 1H19F (virtual 50 Ohm reference: 100.2%/-0.1deg, reflection meter with CRP-Bias capability)
                  PN=Z103203, SN=01267 from 20200402
      Module  2 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111091, SN=00444 from 20200211
      Module  3 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111091, SN=00436 from 20200214
      Module  4 : HPLNA 1H19F (reflection meter with CRP-Bias capability)
                  PN=Z103203, SN=01856 from 20231218
  
- HPLNA 1H19F: HPLNA 1H MODULE 400 Z103203/01267 ECL 06.04
- HPLNA BB31P: HPLNA XBB 31P MODULE 400 Z111091/00444 ECL 04.04
- HPLNA BB31P: HPLNA XBB 31P MODULE 400 Z111091/00436 ECL 04.04
- HPLNA 1H19F: HPLNA 1H MODULE 400 Z103203/01856 ECL 06.06
- RACK: AV4 AQS CHASSIS Z149500/01483 ECL 02.00
- FANTRAY: AV4 AQS FAN TRAY Z149501/01468 ECL 00.02
- PSM-48V: AV4 PSM-48V Z149850/03359 ECL 01.02
- PSM-D: AV4 PSM-D Z149520/01910 ECL 01.01
- REF 1200: AV4 REFERENCE 1200 Z148270/01631 ECL 02.02


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W144057-000097 W144057/000097 ECL 02:
- TCP/IP address = 192.168.99.16
- Firmware VS    = 20210223
- Amplifier      = AV4 BLAH1000 200-600: W144057/000097 ECL 02
- Controller     = BLA CONTROL BOARD 7: W133936/023481 ECL 40
BLA-W144060-000161 W144060/000161 ECL 40:
- TCP/IP address = 192.168.99.13
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABB1000 15-600: W144060/000161 ECL 40
- Controller     = BLA CONTROL BOARD 7: W133936/022594 ECL 21
BLA-W144059-000418 W144059/000418 ECL 10:
- TCP/IP address = 192.168.99.11
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABB500 15-600: W144059/000418 ECL 10
- Controller     = BLA CONTROL BOARD 7: W133936/022679 ECL 21

BSMS: BSMS/2 functionality available
- TCP/IP address = 192.168.99.10
- ELCB firmware version = 20230420
- ELCB = BSMS/2 ELCB: Z100818/08543 ECL 07.02
- Backplane = AV4 BSMS CHASSIS: Z152144/01365 ECL 02.00
- Fan tray = AV4 BSMS FAN TRAY: Z152145/01475 ECL 00.02
- Power Supply = AV4 BSMS PSM-B POWER SUPPLY: Z150090/01420 ECL 00.03
- Power Supply 48V 1 = AV4 PSM-48V: Z149850/03358 ECL 01.02
- Power Supply 48V 2 = AV4 PSM-48V: Z149850/03357 ECL 01.02
- Variable Power Supply 1 = AV4 VARIABLE POWER SUPPLY BD DC-E: Z140144/00261 ECL 01.02
- Power Control = AV4 BSMS POWER CONTROL BOARD: Z150089/01465 ECL 01.00
- SLCB functionality: Available
- Shim System = BOSS1-WB
- SCB channels = 20
- SCB1 = BSMS/2 SCB20: Z102930/13162 ECL 05.00
- Shim matrix file: BOSS1-WB
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z XYZ X3 Y3
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- Lock: Not available
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00826 ECL 05.04
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC-E: Z140144/00261 ECL 01.02
- VTC active channel 1 = BSMS/2 VTA TC-2T: Z119237/05693 ECL 01.00
- VTC accessory channel 1 = BCU II: Z117485/0516 ECL 01.00

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10

- Firmware version = 20231009_1335
MAS Control Unit: MAS_H139288_0790
- TCP/IP address   = 192.168.98.2

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99
Line Distribution Unit 2: PDU2
- TCP/IP address   = 192.168.99.101

LT-MAS: connected via TTY (enabled by user)

Magnet System: BZH 136'40'107H04_D325-89-10638 Z124409/MSC10638 ECL H
- Magnet  : BZH'136'400'107H
- Cryostat: D325'89-10638
- Polarity: SN (Bruker)


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 1 of transmitter 1 (AV4 BLAH1000 200-600 W144057/000097 at TCP/IP 192.168.99.16)
TRX1 AUX  output -> open
TRX2 NORM output -> input 1 of transmitter 3 (AV4 BLABB500 15-600 W144059/000418 at TCP/IP 192.168.99.11)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 2 (AV4 BLABB1000 15-600 W144060/000161 at TCP/IP 192.168.99.13)
TRX3 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLAH1000 200-600 W144057/000097 at TCP/IP 192.168.99.16:
- amplifier 1H-1000W uses blanking 1
- amplifier 1H-100W uses blanking 1

transmitter 2 = AV4 BLABB1000 15-600 W144060/000161 at TCP/IP 192.168.99.13:
- amplifier B-1000W uses blanking 3
- amplifier B-100W uses blanking 3

transmitter 3 = AV4 BLABB500 15-600 W144059/000418 at TCP/IP 192.168.99.11:
- amplifier B-500W uses blanking 2


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 1H19F -> REC1
Tune-TRX2 -> HPLNA BB31P -> REC2
Tune-TRX3 -> HPLNA BB31P -> REC3
Tune-TRX3 -> HPLNA 1H19F -> REC3

