TITLE=MW OFF
Probe: 3.2 mm DNP HCN mode, AVNeo console
Sample: sample 13 HPMC-AS (LF) repeat
Saphire rotor
MAS = 8 kHz, BP = 2660 mB, DP = 1124 mB
Tsample = 120.7 K, flow = 2000 l/h, Heater 0%, Tbearing = 130.1 K, Heater 13.1%, Tdrive = 130.0 K, Heater 10.7%
I = 100 mA
Tcavity = 22.5 C
13C CP echo no filter

1H pulses and SPINAL dec 100 kHz at 67 W, o2 1H offset = -64442 Hz, pcpd2 = 4.8 us
1H CP 100 kHz matched to 13C at 60 W (71 kHz), ramp 70.100.100 on 1H
1 ms CP
L0 = 3
At temp in file 95TITLE_END