##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99138.4mmHXY.30072021.7Li.Li7SiO5Cl/16/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-30 15:49:31.842 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-30 15:40:11.075 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 4664
       00 AD 08 83 60 CD 0C AD A6 83 9C 67 F4 39 32 3F>)
(   2,<2021-07-30 15:51:06.804 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 1050 FT_mod = 6 PKNL = 1 PHC0 = -180.1013 PHC1 = 26.98995 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       4F 9F B0 21 55 1E 1E D7 E1 92 64 82 8B C4 78 45>)
(   3,<2021-07-30 15:51:08.391 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <apk 
       data hash MD5: 8K
       37 3A 4F F0 E6 31 5A AA 16 E5 5D F7 42 11 79 F3>)
(   4,<2021-07-30 15:51:14.424 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <pk fgphup PHC0 = -0.8 PHC1 = 0 
       data hash MD5: 8K
       96 AC FD 9F 64 2B 1C E8 D4 4D 83 3D 59 3C 9C 78>)
(   5,<2021-07-30 15:51:30.021 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Static
       4mm HXY Probe
       sr = -915.53Hz
       90 deg at 2 us ( 83 kHz) at 68 W
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 296 K
       
       
       
       Tsensor = 232.5 K
       gasflow= 700 l/h
       Tsample = 220 K
       
       fwhm = 10400 HzTITLE_END
       data hash MD5: 8K
       96 AC FD 9F 64 2B 1C E8 D4 4D 83 3D 59 3C 9C 78>)
(   6,<2021-07-30 15:52:28.963 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Static
       4mm HXY Probe
       sr = -915.53Hz
       90 deg at 2 us ( 83 kHz) at 68 W
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 296 K
       
       
       
       Tsensor = 215 K
       gasflow= 700 l/h
       Tsample = 200 K
       
       fwhm = 10400 HzTITLE_END
       data hash MD5: 8K
       96 AC FD 9F 64 2B 1C E8 D4 4D 83 3D 59 3C 9C 78>)
(   7,<2021-07-30 15:52:29.160 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li7SiO5Cl
       L7SO5Cl_46
       Static
       4mm HXY Probe
       sr = -915.53Hz
       90 deg at 2 us ( 83 kHz) at 68 W
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 296 K
       
       
       
       Tsensor = 215 K
       gasflow= 700 l/h
       Tsample = 200 K
       
       fwhm = 10400 HzTITLE_END
       data hash MD5: 8K
       96 AC FD 9F 64 2B 1C E8 D4 4D 83 3D 59 3C 9C 78>)
##END=

$$ hash MD5
$$ D5 9D C0 A9 51 CF B8 46 F4 82 DC AB F1 86 30 4A
