##TITLE= Audit trail, TOPSPIN		Version 3.2
##JCAMPDX= 5.01
##ORIGIN= Bruker BioSpin GmbH
##OWNER= benduff1
$$ /opt/topspin3.2/data/benduff/nmr/bd99136.4mmHXHT.27072021.7Li.Li6.5P0.5Si0.5O5Cl/13/pdata/1/auditp.txt
##AUDIT TRAIL=  $$ (NUMBER, WHEN, WHO, WHERE, PROCESS, VERSION, WHAT)
(   1,<2021-07-27 13:47:00.138 +0100>,<benduff1>,<400WB>,<go>,<TOPSPIN 3.2>,
      <created by zg
	started at 2021-07-27 13:46:19.369 +0100,
	POWCHK disabled, PULCHK disabled,
       configuration hash MD5:
       69 34 51 B1 46 DE 81 74 79 C5 5D 33 DA DD 0A 2C
       data hash MD5: 6218
       E4 1A 94 9E AF 52 91 8E A6 3F 20 61 49 F8 44 AE>)
(   2,<2021-07-27 13:49:55.482 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <Start of raw data processing
       efp LB = 120 FT_mod = 6 PKNL = 1 PHC0 = 213.1882 PHC1 = -46.8523 TDeff = 2K SI = 8K 
       data hash MD5: 8K
       03 D9 DF 00 E9 E7 D7 6E 84 2F 4B C5 79 22 E0 70>)
(   3,<2021-07-27 13:50:03.540 +0100>,<benduff1>,<400WB>,<proc1d>,<TOPSPIN 3.2>,
      <pk fgphup PHC0 = -2.2 PHC1 = 0 
       data hash MD5: 8K
       FB 3B E8 DC E3 10 CB 76 79 9B D5 51 11 52 A2 5C>)
(   4,<2021-07-27 13:50:12.294 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.5P0.5Si0.5O5Cl
       L6.5P0.5S0.5O5Cl_17
       Ref Static
       4mm HXHT Probe
       sr = -813.97 Hz
       90 deg at 2.2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 302 K
       
       
       
       Tsensor = 371.3 K
       heater = 1 %
       gasflow= 3000 l/h
       bp = 2500 mbar
       Tsample = 350 K
       
       fwhm = 1250 HzTITLE_END
       data hash MD5: 8K
       FB 3B E8 DC E3 10 CB 76 79 9B D5 51 11 52 A2 5C>)
(   5,<2021-07-27 13:50:12.545 +0100>,<benduff1>,<400WB>,<audit>,<TOPSPIN 3.2>,
      <user comment:
       TITLE=7Li
       Li6.5P0.5Si0.5O5Cl
       L6.5P0.5S0.5O5Cl_17
       Ref Static
       4mm HXHT Probe
       sr = -813.97 Hz
       90 deg at 2.2 us ( 83 kHz) at 126 W
       
       using booster
       
       frame cooling = 70 %
       magnet cooling = 14 turns (full)
       Tshim = 302 K
       
       
       
       Tsensor = 371.3 K
       heater = 1 %
       gasflow= 3000 l/h
       bp = 2500 mbar
       Tsample = 350 K
       
       fwhm = 1250 HzTITLE_END
       data hash MD5: 8K
       FB 3B E8 DC E3 10 CB 76 79 9B D5 51 11 52 A2 5C>)
##END=

$$ hash MD5
$$ C0 19 09 73 3B D5 6E 79 FC C5 02 49 29 C5 79 54
