Galvanostatic charge and discharge measurements were performed using a BioLogic VSP-300 Potentiostat. 
The data was collected in a voltage range of 2.5-4.3 V vs. Li+/Li at room temperature at current density of 5 mA g-1.
The mass load of LiCoO2 is 4.9 mg cm−2.
The data is in .mpr format that is readable in EC-Lab Software which can be obtained at https://www.biologic.net/support-software/ec-lab-software/?utm_source=NL&utm_medium=lien&utm_campaign=EC-Lab_update